The UR-110. Ten years ... and time to say goodbye.

Geneva – October 7, 2021

"While we are not the nostalgic kind here at URWERK, we are proud to be celebrating the 10th anniversary of our 110 collection. This is a creation that won the Best Design prize in the Grand Prix d’Horlogerie de Genève; that faced evil on the wrist of IronMan, the most badass Superhero of them all; and that made the cover of major watchmaking magazines at the time of its launch in 2011. It needed to complete one last mission before it slipped away, so we are going to issue a final UR-110 in bakelite. A one-of-a-kind model that will be auctioned off on our dedicated website, with most of the proceeds going to the Swiss Red Cross", said the two URWERK founders, Felix Baumgartner and Martin Frei.



The UR-110 will therefore be retiring exactly 10 years after its birth – and doing so in style, on behalf of a worthy cause. This one-off UR-110 Bakelite will be unveiled on 10/10 at 10:10 a.m. Geneva time on the <https://urwerkpreowned.com/website>.

The UR-110 Bakelite features a titanium case and an original bezel made of bakelite, a star material from the 1900s. As Felix Baumgartner explains: "Bakelite was one of the first high-tech materials ever developed. Its properties were and remain multiple and revolutionary. Insulating and heat-resistant, it was present in all everyday objects at the time, from eyeglass frames to radios”, Felix Baumgartner.

A couple of dates: The UR-110 Bakelite will be revealed on **10.10.2021 at 10:00 am** Geneva time. The auction will start on October 15th and will close on **17.10.2021 at 10:00 am** Geneva time.

### Technical specifications UR-110 Bakélite. One-of-a-kind model

#### Movement

Calibre: UR 9.01 mechanical, automatic winding

Balance: Monometallic

Jewels: 46

Frequency: 28,800v/h, 4Hz

Balance spring: Flat

Power: Single barrel

Power reserve: 39 hours

Winding system: Uni-directional rotor regulated by double turbines

Finish: Matting, circular graining and diamond-cuts

#### Indications

Satellite complication with rotating hour/minute modules mounted on planetary gears

Control Board: “Day/Night” indicator; “Oil Change” alert for service intervals and small seconds

#### Case

Case in Grade 5 titanium with bezel in Bakélite

Dimensions : 47mm X 51mm X 16mm

Two-position crown with integrated protection.

Water resistance: tested to 3 ATM

Press contact:

Ms Yacine Sar

press@urwerk.com

+41 22 9002027

[www.urwerk.com/press](http://www.urwerk.com/press)